SCOPE OF WORK

SCOPE:F2 JOB NUMBER/CFAS: A028R9W/ A028R9W

PLACE FIBER CABLE AND ASSOCIATED TERMINALS FOR PROJECT LIGHTGIG FIBER TO THE PREM (FTTP) SERVICE FOR PSA 1110PF IN THE MIAMFLAL WIRE CENTER TO SERVE EXISTING COPPER DA(s) 120301 CURRENTLY SERVED BY XBOX(s) AT F 3210 NW 50TH ST .

PERMIT REQUIRED? = YES

PERMIT 1 GRANTOR: City

SWPPP REVIEW IS \*\*NOT\*\* REQUIRED BY EH&S FOR THIS PROJECT BECAUSE IT DOES NOT MEET MINIMUM SWPPP REVIEW THRESHOLDS.

WHAT: FFIB CABLE BEING PLACED ON AUTHORIZATION: N/A /// CFAS: N/A

PFP BEING PLACED ON AUTHORIZATION: PENDING /// CFAS: A02834F

PFP ADDRESS: R 3295 NW 53rd St

WHERE POSSIBLE, ALL PROPOSED FIBER CABLE SHOULD BE PRE-TERMINATED AND FNAP TYPE ORDERED FROM CORNING.

PLACE APPROXIMATELY 0 KF (UPDATE ONCE DESIGNED) OF BURIED\_\_\_\_TBD\_\_\_\_\_ OR SMALLER FIBER CABLE.

PLACE APPROXIMATELY 3261 KF (UPDATED ONCE DESIGNED) OF AERIAL\_\_\_\_\_\_TBD\_\_\_\_OR SMALLER FIBER CABLE.TO SERVE APPROXIMATELY: 145 LU

PLACE THE FOLLOWING MAJOR MATERIAL ITEMS:(CABLES, LENGTHS, ETC)

PLACE THE FOLLOWING TERMINALS: (MSD, QTY)INCLUDES PLACEMENT OF OTHER MINOR MATERIAL ASSOCIATED WITH THE PLACEMENT OF THE MAJOR MATERIAL ITEMS.

TBD

WHERE:PLACE FIBER CABLE AND ASSOCIATED TERMINALS FOR PROJECT LIGHTGIG FIBER TO THE PREM (FTTP) SERVICE FOR PSA 1110PF IN THE MIAMFLAL WIRE CENTER TO SERVE EXISTING COPPER DA(s) 120301 CURRENTLY SERVED BY XBOX(s) ATF 3210 NW 50TH ST ///

PFP COORDINATES: 25.823020 Deg North / -80.250899 Deg W

WHY: THE FOLLOW DA(s): 120301 IS/ARE IDENTIFIED AND APPROVED FOR PROJECT LIGHTGIG TO PLACE A PFP AND OVERLAY WITH FIBER DISTRIBUTION CABLE.

WHY THIS WAY: THIS PROJECT IS DESIGNED PER APPLICABLE CLR GUIDELINES.

WHY NOW:PROJECT IS ALIGNED WITH LIGHTGIG TRACKING REPORT WPC04

\*\*\*SPECIAL NOTES AND CONSIDERATIONS\*\*\*N/A